<html>

<head>
<meta HTTP-EQUIV="Content-Type" CONTENT="text/html; charset=windows-1250">
<meta NAME="GENERATOR" CONTENT="Microsoft FrontPage 3.0">
<title>Calculation of water injecting into steam conditioning station</title>
<meta NAME="Template" CONTENT="C:\Program Files\Microsoft Office\Office\html.dot">
</head>

<body LINK="#0000FF" VLINK="#800080" bgcolor="#FFFFFF">
<p style="background:black;"><img src="Ventily_help_all.jpg"></p>

<p><big><font FACE="Arial">Calculation of water injecting into steam conditioning station</font></big></p>
<font FACE="Arial" SIZE="2">

<p></font><u><font FACE="Arial" size="3">Calculation conditions:</font></u><font
FACE="Arial" SIZE="2"></p>
</font>

<p><font FACE="Arial" SIZE="2">Ideal isoentalpic continual intermixture is supposed to
occur.<br>
Medium with index 1 - superheated steam<br>
Medium with index 2 - cooling water designed for inecting<br>
Medium with index 3 - cooled mixture at steam conditioning´s (cooler´s) outlet<br>
Input data:<br>
&nbsp;&nbsp;&nbsp; Pressure (MPa abs) and medium temperature (°C) for all three states
(steam, water, mixture)<br>
&nbsp;&nbsp;&nbsp; Qunatity of steam to be cooled Q1 or quantity of mixture Q3 (kg/h)<br>
Used units<br>
&nbsp;&nbsp;&nbsp; Pressure - overpressure or absolute value<br>
&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp; - Mpa, bar, atm, kPa<br>
&nbsp;&nbsp;&nbsp; Flow&nbsp;&nbsp;&nbsp; - in unit of weight<br>
&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp;&nbsp; - kg/h, t/h, kg/s<br>
&nbsp;&nbsp;&nbsp; Temperature - °C, K, °F<br>
Calculation results determine quantity of injecting water Q2 necessary for cooling given
superheated steam quantity to required temperature.</font></p>
</body>
</html>
