<html>

<head>
<meta HTTP-EQUIV="Content-Type" CONTENT="text/html; charset=windows-1250">
<meta NAME="GENERATOR" CONTENT="Microsoft FrontPage 3.0">
<title>Other liquid</title>
<meta NAME="Template" CONTENT="C:\Program Files\Microsoft Office\Office\html.dot">
</head>

<body LINK="#0000FF" VLINK="#800080" bgcolor="#FFFFFF">
<font FACE="Arial">

<p style="background:black;"><img src="Ventily_help_all.jpg"></p>
</font>

<p><big><font FACE="Arial">Other liquid</font></big></p>

<p><u><font FACE="Arial" size="3">Calculation conditions :</font></u></p>

<p><font FACE="Arial" size="2">Medium is in state of liguid. Turbulent flowing is supposed
to occur (Re &gt; 10000) . Calculated Kvs value applies to state when cavitation does not
occur. Effect of medium viscosity is ignored in calculation.<br>
Following data must be entered for calculation of valve´s Kvs value:<br>
&nbsp;&nbsp;&nbsp; Inlet pressure p1<br>
&nbsp;&nbsp;&nbsp; Outlet pressure p2 or differentila pressure dp<br>
&nbsp;&nbsp;&nbsp; Flow Q <br>
&nbsp;&nbsp;&nbsp; Medium temperature t <br>
&nbsp;&nbsp;&nbsp; Medium density in given temperature<br>
Calculation is executed as same as for water, but the medium density for given temperature
must be entered in addition to imput data. Further these data can be saved in database of
other liquids for repetitional using (for more details see: Updating service and data
tables utilization).<br>
If the liquid´s satuarted steam pressure is entered for given temperature, then checking
of cavitation is executed, otherwise such checking is not executed at all.</font></p>
</body>
</html>
